# q2ew Configuration File Commands

(last revised 31 March 1999)
Page Index:
1. Example configuration file
2. Functional command listing
3. Alphabetic command listing & description
4. Descriptor file example

On startup, q2ew reads the configuration file named on the command line. As always, the configuraton file contains comments:

>     #  marks the line as a comment (example: # This is a comment).

Command names must be typed in the control file exactly as shown in this document (upper/lower case matters!). q2ew supports one diagnostic command line option, -v is for verbose mode so that you can see packets coming in.

## 1. EXAMPLE CONFIGURATION FILE

    #
    # q2ew configuration file
    #
    # This code receives MiniSEED records from COMSERV, converts them into
    # Earthworm trace buf messages, and stuffs them into a wave ring.
    #
    #
     ModuleId	MOD_Q2EW	# module id for this import,
     RingName	WAVE_RING	# transport ring to use for input/output,

     HeartbeatInt	10		# Heartbeat interval in seconds
    				# this should be half the q2ew.desc heartbeat!

     LogFile	1		# If 0, don't write logfile at all,

     LOG2LogFile 	1		#  write LOG chans to log file
    				# this is useful for debugging timing or
    				# data logger problems.

    TimeoutNoSend	5		# If no data for X seconds from COMSERV for
    				# ALL stations,  then kill process (HB and
    				# main thread).
    				# NOTE: this timeout does not take effect until
    				# a trace data packet comes from comserv. That
    				# is, LOG channels do not count!
    				#
    				# Iff TimeoutNoSend == 0, then this data
    				# check is DISABLED and q2ew will only die
    				# if EW or COMSERV dies.

    # For ATWC, set this next config param to CSQ_LAST
     ComservSeqBuf	CSQ_LAST	# This is a comserv sequence control value
    				# that can have the following settings:
    				# CSQ_NEXT  = Get newer than already received
    				# CSQ_LAST  = Get first available data (latest)
    				# CSQ_FIRST = Get all data in DAQ
    				# This effects what data are returned.

    # These are optional for those EW users who want to have a pin number
    # instead of a SCN. The keyword here is SCN2pinmap. No duplicate checking
    # occurs

    # Example
    #		S	C    	N	pin
    SCN2pinmap 	Q003	HHZ  	AT	1
    SCN2pinmap 	Q003	HHN  	AT	2
    SCN2pinmap 	Q003	HHE  	AT	3

## 2. FUNCTIONAL COMMAND LISTING

Below are the configure commands recognized by q2ew, grouped by the function they influence. Most of the commands are required. Only SCN2pinmap and LOG2LogFile are optional.

             Earthworm system setup:
     		MyModuleId	   	required
    		RingName	   	required
    		ComservSeqBuf	   	required
    		HeartbeatInt	   	required
    		TimeoutNoSend	   	required

    	Output Control:
    		LogFile		   	required
    		LOG2LogFile		optional
    		SCN2pinmap		optional

## 3. ALPHABETIC COMMAND LISTING & DESCRIPTION

In the following section, all configuration file commands are listed in alphabetical order. Listed along with the command (bold-type) are its arguments (in red), the name of the subroutine that processes the command, and the function within the module that the command influences. A detailed description of the command and is also given. Default values and example commands are listed after each command description.

    command arg1				processed by		function

    ComservSeqBuf csqtype			main			Main q2ew Thread

> This command is used to define how q2ew gets data from COMSERV. csqtype is the name of a #define as found in COMSERV's comserv/include/service.h file. csqtype can have the following values:

>     	CSQ_NEXT
>     	CSQ_LAST
>     	CSQ_FIRST

> CSQ_LAST is what is being used for ATWC since they are only interested in the latest available data from the digitizer or DA (digitizer=DA in Quanterras documents). CSQ_NEXT gets only the data that are newer than that already receieved by COMSERV and CSQ_FIRST gets all the data in the DA's buffer.

>     Default:  none
>     Example:
>     	ComservSeqBuf CSQ_LAST

    HeartbeatInt beat			HeartBeat		Earthworm setup

> Beat the q2ew heart every beat seconds. This is implemented as a separate thread in q2ew.

    LOG2LogFile switch			logLOGchans 		Main q2ew Thread

> Sets the on-off switch for writing Quanterra LOG channels to the LogFile. If switch is 0, no LOG channels will be written to the log. If switch is 1, q2ew will write all LOG channels to the LogFile. Turning this on will automatically turn on writing of a LogFile.

>     Default:  0 - do not use logit() for LOG channels

    LogFile switch				GetConfig		Earthworm Setup

> Sets the on-off switch for writing a log file to disk. If switch is 0, no log file will be written. If switch is 1, q2ew will write a daily log file(s) called q2ewxx.log_yymmdd where xx is q2ew's module id (set with "MyModuleId" command) and yymmdd is the current UTC date (ex: 960123) on the system clock. The file(s) will be written in the EW_LOG directory (environment variable).

>     Default:  none

    MyModuleId mod_id			GetConfig		Earthworm setup

> Sets the module id for labeling all outgoing messages. mod_id is a character string (valid strings are listed in earthworm.d) that relates (in earthworm.d) to a unique single-byte number.

>     Default:  none
>     Calnet:   MyModuleId MOD_Q2EW

    RingName ring				GetConfig		Earthworm setup

> This is the ring into which the waveforms and messages are sent.

>     Default:  none, required option
>     ATWC:   RingName WAVE_RING

    SCN2pinmap S C N pin			insertSCN		Main q2ew Thread

> This command is used to define how q2ew maps a Station Channel Name to a pin number for those installations who wish to define pins....This is a throwback to old digitizers and is not recommended since Quanterra digitizers can properly be configured to know SCN information. Data from S C N is compared to the SEED header of the waveform packets coming off the DA and the pin number is substituted into the tracebuf struct passed to Earthworm. S is for station name, C is for channel identifier, and N is for network code. Note that station, channel, and network names in Quanterra follow the SEED convention and can be 5, 3, and 2 chars in length respectively.

>     Default:  none, optional command
>     SCN2pinmap	Q003 HHZ AT  1
>     SCN2pinmap	Q003 HLN AT  2
>     SCN2pinmap	Q003 HLE AT  3

    TimeoutNoSend timeout			HeartBeat		Earthworm setup

> If no waveform packets come from the DA after timeout seconds, the q2ew module will notify statmgr and die. If timeout is set to 0, then the q2ew module will never check for this timeout. If set to 0, q2ew will only die if COMSERV dies, or if the Earthworm system calls for its termination. This timeout begins once the first Waveform packet is received from ANY DA served by COMSERV. It is not specific to any one DA.

>     Default:  none, required option
>     ATWC:   TimeoutNoSend 0

## 4. DESCRIPTOR FILE EXAMPLE

Here is a copy of the q2ew.desc file as implemented. Note that all causes of death for q2ew feed through the function q2ew_die() which logs all causes of death using logit() and sends a message to the statmgr utility.

    modName  q2ew
    modId    MOD_Q2EW
    instId   INST_ATWC

    restartMe	# restart this sucker as it is critical to data collection
    #
    #
    #    Heartbeat Specification.  If the status manager does not receive
    #    a heartbeat message every  seconds from this module, an
    #    error will be reported (client module dead).   is the maximum
    #    number of pager messages that will be reported and  is the
    #    maximum number of email messages that will be reported.  If the
    #    page or mail limit is exceeded, no further errors will be reported
    #    until the status manager is restarted.
    #
    tsec: 20  page: 0  mail: 99

    # these are the statmgr messages that q2ew will send before dieing
    #
    err: 0  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "COMSERV has a problem and died"
    #
    err: 1  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "COMSERV Recv NO DATA TIMEOUT and died"
    #
    err: 2  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "SIGNAL caused q2ew to die"
    #
    err: 3  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "EW tport_putmsg() failed, q2ew dead"
    #
    err: 4  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "EW TERMINATE recv'd, q2ew dead"
    #
    err: 5  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "EW config problems on startup, q2ew dead"
    #
    # BELOW: WARNINGS, NOT FATAL YET
    err: 6  nerr: 1  tsec: 0  page: 5  mail: 20
    text: "qlib2 decompression errors"
    #

Module Index | q2ew Overview