
                libslink: the SeedLink client library

                              4 May 2004

Purpose:

	The purpose of this library is to provide all needed functionality
for communicating with a SeedLink server in a generalized way.  This library
facilitates rapid SeedLink client development as the client does not need
to know any details of the SeedLink protocol.  The library is intended to
work with all existing versions of SeedLink and will not use features that
a given SeedLink server does not support.  The library is written in C.


Threads:
	
	The library is thread-safe on Unix-like platforms as long as
each thread manages it's own SeedLink Connection Description (see
below).  The library is definitely not thread-safe under Win32.


Usage:

-------------------  The SeedLink Connection Description -------------------

	The usage philosophy is that a so-called SeedLink Connection
Description (SLCD) stipulates all aspects of a connection to a server. In
libslink the SLCD is implemented as a C struct which is used by most of the
utility functions.  The struct is given below with descriptions of each
parameter:

  typedef struct slcd_s
  {
    SLstream   *streams;
    char       *sladdr;
    char       *begin_time;
    char       *end_time;

    short int	resume;
    short int   multistation;
    short int   dialup;
    short int   lastpkttime;
    short int   terminate;

    int         keepalive;
    int         netto;
    int         netdly;

    float       protocol_ver;
    char       *info;
    int         link;
    SLstat     *stat;
    SLlog      *log;
  } SLCD;


Parameter descriptions:

  streams:	A pointer to struct that specifies streams to be 
		requested from the server; this is the beginning of the
		"stream chain".  The user should not need to interface
		directly with the stream chain as there are helper functions
		to populate the chain; namely sl_addstream() and
		sl_setuniparams().

  sladdr:	The address of the SeedLink server to connect to in 
		'host:port' format.  example: "st27.gfz-potsdam.de:18000".
		
  begin_time:
  end_time:	If these parameters are set the connection is configured
		for time window extraction.  The end_time is optional.  When
		no end_time is set the behavior is server dependent but can
		be expected, with current server versions, to indicate that
		the server should keep the window open-ended and not close
		the connection.  The format is 'year,month,day,hour,min,sec',
		i.e. "2002,05,03,13,00,00", for both parameters.  If
		these parameters are set they will override the use of any
		sequence numbers (specified in the stream chain) to resume
		a data stream.

  resume:	A flag to control the inclusion of sequence numbers with the
		DATA or FETCH commands.  If this flag is true sequence numbers
		will be appended to the DATA/FETCH command instructing the
		remote server to start sending data from the supplied sequence
		number for a given stream.  If false no sequence numbers will
		be sent and the server will start the stream from the next
		arriving data packet.  The default is 1 (true).

  multistation: A flag to indicate that the connection should be configured
		in multi-station mode.  If you use sl_addstream() or 
		sl_setuniparams() to populate the stream chain this
		parameter is set automatically.  The default is 0 (false).

  dialup:	A flag to indicate that the connection should be configured
		in so-called dial-up mode.  This is a mode of  operation
		where the server will close the connection when the end of
		the selected buffers have been reached, i.e. the most current
		data has been sent.  The default is 0 (false).

  lastpkttime:  A flag to indicate if the last packet time should be appended
                to a DATA or FETCH command during connection negotiation.
		The last packet time is only (optionally) sent to SeedLink
		servers version 2.93 or greater.  In combination with the last
		packet sequence number, this information is used by the remote
		server to decide if the last packet sequence number is valid
		for the current buffer.  Basically this should prevent large
		amounts of overlap data from being sent if the client has not
		been connected in a while and is a basic sanity check.  The
		default is 0 (false).

  terminate:    A flag to indicate that the connection to the remote server
		should be shutdown and the internal buffer should be flushed
		of complete packets.  The routine sl_terminate() will set this
		flag; it is recommended to use sl_terminate() in a signal
		handling routine.  The default is, of course, 0 (false).

The following parameters have specific meaning for the connection
management function described below, sl_collect():

  keepalive:	Interval, in seconds, to send keepalive requests to the
		server.  Default is 0 (disabled).

  netto:	Network timeout, in seconds.  If no packets are received
		within this period the connection will be closed and
		re-opened.  Default is 600 seconds.  A value of 0 disables
		this feature.

  netdly:       Network connection delay, in seconds.  This parameter
		controls how much time the manager will wait until attempting
		to re-connect.  Default is 30 seconds.

The following parameters are maintained by the library routines and should
not be changed by the calling program:

  protocol_ver: This is the version of the SeedLink protocol in use.  This
		value is parsed from the server's response to the
		HELLO command and will be set to 0.0 when the version
		could not be detected.  Internal library routines use
		this value to check if specific features should be
		used with the currently connected server.  If the
		version could not be detected the default action is to
		allow all features.  The first line of response to the
		HELLO command is expected to be in the format:
		"seedlink v#.# <optional text>" where 'seedlink' is
		case insensitive and '#.#' is the protocol version.

  info:         This parameter indicates that an INFO packet should be
		requested from the server during the next call to
                sl_collect().  The client should request INFO packets via
		the sl_request_info() function and not use this value
		directly.

  link:		This is the file descriptor associated with the connected
		network socket.  This value will be -1 when not connected
		to a server.


-----------   Configuring the SeedLink Connection Description   ------------

There are a number of functions to assist with the creation of a SLCD (see
the man pages for programming details):

  sl_newslcd()  : allocate and initialize a SLCD struct with default values.

  sl_freeslcd() : free all memory associated with a SLCD.

  sl_addstream() : add a stream entry to the stream chain; multi-station
	mode is implied.

  sl_setuniparams() : set the stream parameters for uni-station mode.

  sl_read_streamlist() : read a list of streams from a file and add them
	to the stream chain; multi-station mode is implied.

  sl_parse_streamlist() : parse a list of stream from a string and add them
	to the stream chain; multi-station mode is implied.


--------------------   Using the connection manager   ----------------------

A function is provided to manage a connection to a SeedLink server based on
the parameters in the connection description.

  sl_collect() : using the parameters in the connection description this
	function will maintain a persistent connect to a server.  Designed
	to run in a tight loop at the heart of a client program this
	routine blocks until a packet is received, then setting the slpack
	pointer to the packet and returning a positive integer.  Zero (0) is
	returned when either 1) the requested time window has been
	fulfilled, 2) the termination sequence is completed or 3) an error
	occurred.

	If the 'info' parameter is set in the connection description the
	manager will request the specified INFO during the next iteration
	of sl_collect().  In-stream INFO requests can be made by using
	the sl_request_info() function.

	The manager uses the keepalive, netto and netdly parameters in the
	way specified above.

  sl_collect_nb() : This is a non-blocking version of sl_collect() it will
	always return whether a packet is received or not.  If not
	called at regular short intervals this function might not be
	able to properly manage the connection, i.e. update internal
	timers for timeouts, send keepalives, etc.  For this reason
	this is NOT A RECOMMENDED INTERFACE.  If you really need to
	use this function try to call it at regular intervals, in
	other words, don't spend too much time processing or sleeping
	in-between calls.

  sl_terminate() : set the terminate flag in the connection description.
	This will cause sl_collect() to close the network connection, 
	finish passing received packets to the caller and finally return 0.

It is highly recommended to implement signal handling to call 
sl_terminate() for smooth program termination.


------------------------   Using state files   -----------------------------

The state of each stream, the sequence number and time stamp in the stream
chain, can be saved to and recovered from state files:

  sl_savestate() : save current sequence numbers and time stamps to a file.

  sl_recoverstate() : recover sequence numbers and time stamps from a file.

Using these functions a SeedLink client can be shut down and re-started
without a gap in the data stream as long as all necessary data still exists
in the SeedLink buffer.


-----------   Controlling output from the library functions   --------------

All of the log and diagnostic messages emitted by the library functions
use the same interface.  The output from this interface can be controlled.
This is useful when the library will be embedded in a larger system with
a custom logging facility.  See the man page for more details.

  sl_loginit() : initialize the verbosity level of the library
	functions, also set the functions and prefixes used for log,
	diagnostic and error messages.

  sl_log() : the central logging facility.  Behavior is controlled by the
	settings specified with sl_loginit().

The default destination for log messages is standard output (stdout),
while all diagnostic (including error) messages go to standard error
(stderr).  Most of the internal messages emmited by the library are
considered diagnostic and will, by default, go to standard error.

The default prefix for log and diagnostic messages is nothing. The
default prefix for diagnostic error messages is "error: ".

There are reentrant versions of these functions that operation either on the
logging parameters in a SLCD or directly on a logging parameter SLlog struct.
They are intended for use in threaded programs or where a complex logging
scheme is desired.  See the man pages for more details.


-------------------   Handling of Mini-SEED records   ----------------------

Some functions are included for parsing Mini-SEED record headers and
unpacking/decompressing data samples.  As of version 1.0 the data
formats supported are INT-16, INT-32, Steim-1 and Steim-2.

  msr_parse_() : parse the fixed section data header and blockettes
	100, 1000 and 1001.  Optionally unpacking/decompressing data samples.

  msr_print() : print header values out using sl_log().  The level of
	information printed can be controlled.

There are also functions to return the (double precision) sample rate and
the record start time as a (double precision) POSIX epoch, these are
msr_dsamprate() and msr_depochstime() respectively.  Consult the manual
pages for further details.


--------------------   Illustrative program example   ----------------------

For a real example of libslink usage see the program in the 'example'
directory.  Below is a simple, step-by-step, schematic view of common library
usage:

  sl_newslcd()          - initialize new connection description.
    - set a server address
    - set other desired parameters; begin/end time or dialup
  sl_parse_streamlist() - parse a stream list string
  sl_recover_state()    - recover state information from a file

  while ( sl_collect() != 0 )
    {
       sl_packettype();
       sl_sequence();

       [ do something with the data record ]

    }

  sl_savestate()        - save state information to a file
  exit


