#
Fir Configuration File

(last revised 12 December, 2008)

    #

    #                     Configuration File for Fir

    #

    MyModId          MOD_FIR

    InRing           WAVE_RING       # Transport ring to find waveform data on,

    OutRing          WAVE_RING       # Transport ring to write output to,

                                     # InRing and OutRing may be the same.

    HeartBeatInterval     30         # Heartbeat interval, in seconds,

    LogFile            1             # 1 -> Keep log, 0 -> no log file

    #Debug		 		 # Write out debug messages (optional)

    MaxGap              1.5         # Maximum gap, in sample periods, allowed

                                    # between trace data points.

                                    # When exceeded, channel is restarted.

    # Specify the filter frequency response characteristics with two or more

    # commands fo the form: Band

    #

    # where:

    #   f_low = low frequency limit of a band

    #   f_high = high frequency limit of a band

    #   level = desired level of the band: 1 for pass band, 0 for stop band

    #   deviation = amount of ripple allowed from desired level

    #

    # All frequencies specified must be in the range 0.0 - 1.0, where 1.0

    # corresponds to the Nyquist frequency. (Nyquist frequency is half the sample

    # rate and is the maximum frequency content that can be in a time series.)

    # One band must start at 0.0 frequency; one band must end at 1.0 frequency. Any

    # number of additional bands may be specified (up to a total of ten bands.)

    Band 0.0 0.3 1 0.005

    Band 0.4 1.0 0 0.005

    # If you want Fir to compute and log its filter coefficients and then

    # exit, specify "TestMode".

    #TestMode

    #

    # Specify logos of the messages to grab from the InRing.

    # TYPE_TRACEBUF is assumed, therefore only module ID and

    # installation ID need to be specified

    #

    GetWavesFrom    INST_WILDCARD MOD_WILDCARD  # TYPE_TRACEBUF (assumed)

    #

    # List SCNL codes of trace messages to fir and their output SCNL codes

    # Wildcard characters are not allowed here.

    #

    #        IN-SCNL     OUT-SCNL

    GetSCNL TEST EHZ UW --  TEST EWZ UW --

Module Index | Fir Overview