# SaraAdSend Configuration File for Earthworm 7.2

## For the *******

Created Nov 16, 2007 by Larry Cochrane (Webtronics)

Below is a typical SaraAdSend.d configuration file. This file should be located in the \earthworm\run\params directory. The ModuleId must be added to the earthworm.d file also located in this directory.

    #

    #                    CONFIGURATION FILE FOR SARAADSEND

    #                    -----------------------------

    ModuleId         MOD_SARAADSEND_A       # Module id of this instance of SaraAdSend

    OutRing          WAVE_RING              # Transport ring to write waveforms to

    CommPort         1                      # Comm port number

    PortSpeed        38400                  # Comm port baud rate, can be set to 9600, 19200, 38400 or 57600

    #

    #                        CHANNEL CONFIGURATION

    Nchan            3                      # Specify number of channels to record, can 1 to 8

    ChanRate         100                    # Sampling rate in samples per second, can be 5, 10, 20, 50, 100 or 200

    #

    #                         TIMING INFORMATION

    HeartbeatInt     15                     # Heartbeat interval in seconds

    TimeoutNoSend    30                     # Time in seconds before program will reset if no data from ADC board

    TimeoutNoSynch   60                     # Not used

    UpdateSysClock   0                      # 1 = PC time updated with AD board time

    HighToLowPPS     0                      # 1 = PPS signal direction is High to Low

    TimeOffset       0                      # Time Reference offset in milliseconds

    #

    # Time Reference Types:

    # 0 = Use PC Time, 1 = Garmin GPS 16 or 18, 2 = Motorola ONCORE NMEA,

    # 3 = Motorola ONCORE Binary, 4 = WWV (must have WWV option on the ADC board )

    #

    TimeRefType      0                      # One of the types above

    TimeFilePath     c:\earthworm\          # where to place the time.dat file

    #

    #

    #                          OTHER INFORMATION

    LogMessages      1                      # 1 = Log messages from DLL & ADC to log file

    NoPPSLedStatus   0                      # 1 = Disable 1PPS LED blinking

    AdcDataSize      2                      # ADC trace buffer data size in bytes. Can be 2 or 4 bytes

    #

    #

    #               SCNL (Station/Component/Network/Location) FOR EACH ADC CHANNEL

    # Chan lines must follow the Channel Configuration lines in this file. There should

    # be Nchan (see above) SCNL lines.

    #

    #     Chan  Station/Comp/Network/Location

    #   -------   --------------

    Chan    0       STA BHZ PN NC

    Chan    1       STA BHN PN NC

    Chan    2       STA BHE PN NC

    #-----------------------------

    #

SaraAdSend Overview