# Import_ida Configuration File

(last revised 17 March 1998)

    # @(#)import_ida.d	1.1 12/26/97

    # import_ida parameter file

    #  Basic Earthworm setup:

    MyModuleId         MOD_IMPORT_IDA # module id for this process

    OutRing            WAVE_RING      # output ring

    HeartBeatInterval  30             # seconds between heartbeats

    # We need to assign unique pin numbers to each net/sta/chan triple that

    # gets sent to the output ring.  Give the name of the file that contains

    # this information.  The format of this file must be the same as what

    # pick_ew expects.  You can create your own file with IDA specific

    # entries (see ida.sta for an example), or you can add the required

    # information to the pick_ew station file.  The picker parameters are

    # not required here, and as far as this program is concerned those fields

    # may be left blank.

    PinnoFile          ida.sta

    # It is up to the user to insure that there are entries in the above file

    # for all expected net/sta/chan triples, however the program will work even

    # if the database is incomplete.  In such a case, an unresolved net/sta/chan

    # will be assigned a default pin number of 12345.  You can override this

    # default by specifying an alternate value.

    DefaultPinno       12345

    # Define the policy to follow when reconnecting after circuit timeouts.

    # There are two choices: MINIMAL_GAP, or MINIMAL_DELAY.  If the former

    # is selected then the program will request the flow start at the end of

    # whatever has been received so far.  If the latter is selected then the

    # program will request the flow start with the most recent packet available

    # on the server.

    Policy             MINIMAL_DELAY

    # The network code for Project IDA stations is II, and that is the default

    # code which gets loaded into the packet headers.  If you want to override

    # this with some other code, enter it here.

    Network            II

    # List the server(s) and stream(s) that are desired.

    # The station channel specifications should follow the syntax

    # described in ftp://idahub.ucsd.edu:/pub/pickup/idatap-1.2.1.tar.Z

    #

    # You can give either the fully qualified host name, or its IP address

    # in the usual decmial dot notation (eg, 111.22.333.44)

    #

    #          Hostname              Station/channel list

    server   nnn.xxx.mmm.5        nna:bhz+pfo:bhz+sur:bhz

Module Index | Import_ida Overview