##

U. C. Berkeley Seismograph Station

Date: March 24, 1998

### Location, Contact, and Address:

Univ. Calif. Berkeley

Contact: Doug Neuhauser

### Network Characteristics

Digital Broadband stations in northern California.

###

Earthworm Modules under development

- Use binder to associate events from BDSN Murdock-Hutt detector messages, which are imported as EW picks (pick2 format). Developed MHH->Pick import module.
- Experimental 3-component broadband phase detector module.
- Exchange waveforms between BDSN and NCSN using binary import/export. Developed a comserv/ew module for MiniSEED->EW waveform import.
- Developed EW MiniSEED waveform format and import procedure for MiniSEED waveform data.
- Utilize EW rings for monitoring hearbeats of various aspects of REDI processing.

Return to main Earthworm or Sites pages.