#
Heli_ew Configuration File

(last revised August 10, 1999)

    #
    # This is the heli_ew parameter file. This module gets data gulps
    # from the waveserver(s), and creates helicorder displays.

    #  Basic Earthworm setup:
    #
    LogSwitch    1              # 0 to completely turn off disk log file
    MyModuleId   MOD_HELI       # module id for this instance of report
    RingName     HYPO_RING      # ring to get input from
    HeartBeatInt 15             # seconds between heartbeats

    # List the message logos to grab from transport ring
    #             Installation     Module        Message Type
    GetSumFrom    INST_WILDCARD    MOD_EQPROC    TYPE_HINVARC

    wsTimeout 12 # time limit (secs) for any one interaction with a wave server.

    # List of wave servers (ip port comment) to contact to retrieve trace data.
     WaveServer aaa.bbb.ddd.eee 16022      "wsv2 - ad1"
     WaveServer aaa.bbb.ddd.fff 16023      "wsv2 - ad2"

    # List of target computers/directories to place output.
    #       UserName  IP Address            Directory
    Target myname@webserver1:/home/www/waveforms/helicorder/
    Target myname@webserver2:/home/www/waveforms/helicorder/

    # Filename prefix on target computer.  This is useful for identifying
    # files for automated deletion via crontab.
    Prefix nc

    # Directory in which to store the temporary .gif, .link and .html files.
    GifDir   /home/bigfiles/GIFs/helicorder/

    # Plot Parameters - sorry it's so complex, but that's the price of versatility
            # The following is designed such that each SCN creates it's own
            # helicorder display; one per day of data.
    # S                  Site
    # C                  Component
    # N                  Network
    # 04 XSize           Overall size of plot in inches
    # 05 YSize           Setting these > 100 will imply pixels
    # 06 Minutes/Line    Number of minutes per line of trace
    # 07 Gain Factor     Instrument gain in microvolt/bit.
    # 08 Scale Factor    Scale factor to dress up image.
    # 09 Plot Previous   On startup, retrieve and plot n previous hours from tank.
    # 10 Local Time Diff UTC - Local.  e.g. -7 -> PDT; -8 -> PST
    # 11 Local Time Zone Three character time zone name.
    # 12 Show UTC        UTC will be shown on one of the time axes.
    # 13 Use Local       The day page will be local day rather than UTC day.
    # 14 Mean Removal    Mean of 1st minute of each line will be removed.
    # Comment            A comment for the top of the display.
    #
    #     S    C   N  04  05  06 07   08   09  10  11   12 13 14  Comment

     Plot MSL  VHZ NC 10  20  15 1.0  1.0  1   -7  PDT  1  0  1   Mammoth
     Plot HSF  VHZ NC 10  20  15 0.5  1.0  1   -7  PDT  1  0  1   "San Juan Bautista"
     Plot GPM  VHZ NC 10  20  15 0.5  1.0  1   -7  PDT  1  0  1   "Geysers"
     Plot KRP  VHZ NC 10  20  15 0.25 1.0  1   -7  PDT  1  0  1   "Cape Mendocino"
     Plot JSF  VDZ NC 10  20  15 6.8  1.0  1   -7  PDT  1  0  1   "Bay Area DST"
     Plot JSG  VDZ NC 10  20  15 1.0  1.0  1   -7  PDT  1  0  1   "Bay Area Nano"

        # *** Optional Commands ***

     Days2Save     7    # Number of days to display on web page; default=7
     UpdateInt    10    # Number of minutes between updates; default=2
     RetryCount    2    # Number of attempts to get a trace from server; default=2
     Logo    smusgs.gif # Name of logo in GifDir to be plotted on each image

    # We accept a command "SaveDrifts" which logs drifts to GIF directory.
      SaveDrifts

    # We accept a command "Debug" which turns on a bunch of log messages
    # Debug
    # WSDebug

Module Index | Heli_ew Overview