#
Import_generic Configuration File

(last revised May 13, 2000)

## 1. EXAMPLE CONFIGURATION FILE

    #
    # import_generic configuration file
    #
    # This is the companion receiver for export_generic and export_scn. It
    # initiates a connect request to the export specified in this file. It
    # will accept any legal message from the export it connected to, and put
    # it into the ring it's attached to. The logo of the message will the same
    # as it was in the originating system.
    # If the heartbeat string it receives doesn't match, it will quit operations.
    # If the expected heartbeat is not received within "SenderHeartRate" seconds,
    # it will re-initialize the connection.
    #Background:
    # Import/Export are the long-distance message transfer
    # modules. They operate as one-on-one pairs. There are two variants of
    # export: export_generic, which ships messages with specified logos, and
    # export_scn which ships only trace data, but with specified SCN names.
    #
    # Import/Export send heartbeats to each other, as well as into their
    # local earthworm systems. If the heartbeat from the distant partner is
    # not received whithin the expected time period (RcvAliveInt) the link is
    # terminated, and an attempt to reconnect is initiated. If things go
    # seriously wrong, the heartbeat into the local earthworm system in
    # stopped. The expectation is that "restartMe" has been set in the .desc
    # file, and we'll be killed and restarted.
    #
    # All socket operations are performed with a timeout. This is noramlly
    # defaulted, but can be set in this file (SocketTimeout).
    #
    # Export maintains a circular FIFO buffer of messages to be shipped. The
    # size of this buffer (RingSize) controls the maximum latency of the
    # data.
    #
    #
    #Configuration notes:
    #
    # "restartMe" should be stated in our desc file.
    #
    # The period of our local heartbeat (HeartBeatInt) must be safely smaller
    # (faster) than our advertised period in our .desc file (tsec:).
    # Otherwise we'll get continually restarted for no good reason.
    # Note that tsec:0 implies no heartbeats expected, and so we'll never get
    # restarted.
    #
    # The rate at which we send heartbeats to our distant partner should be
    # considerably faster than the rate at which our partner expects them.
    # Otherwise, a heartbeat delayed in transmission will cause our partner to
    # conclude that the link is broken, and cause them to break the link and
    # reinitialize. Which will cause us to do the same.
    #
    # For export, the ServerIPAdr is  the address of the port to be used in
    # the exporting machine.  This is to specify a network card case the
    # exporting machine has several network cards.
    #
    # If SocketTimeout is specified, it should be at least as large as the
    # expected period of heartbeats from our distant partner.
    #

     MyModuleId     MOD_IMPORT_GENERIC   # module id for this import,
     RingName       PICK_RING            # transport ring to use for input/output,
     HeartBeatInt   120                  # Heartbeat interval in seconds
    #                                     Should be >= SenderHeartRate
     LogFile        1                    # If 0, don't write logfile at all,

     MaxMsgSize     65000      	# maximum size (bytes) for input/output msgs
    # Note: If an oversized message is received, it will be discarded, the
    #       socket will be closed, log an error, and it will connect and try
    #	again.

     MyAliveString  "MenloAlive"	# heartbeat text to foreign server machine
     MyAliveInt     120      	# seconds between alive msgs sent to server
    				# 0 => no alive messages to sending machine

    # Sender description follows:
    SenderIpAdr	aaa.bbb.c.ddd	# Ip address of the machine we're to listen to
    SenderPort	16005		# IP port number used by sender
    SenderHeartRate	60		# Sender's heart beat interval in seconds
    				# 0 => no heartbeat expected
    SenderHeartText    "alive"	# Sender's heartbeat text

    # Optional commands:

    #SocketTimeout 60000 #Timeout for Socket_ew calls in milliseconds
                         #Should be atleast the SenderHeartRate
    	       	     # Will default to SenderHeartRate
    #HeartbeatDebug 0    #Change this to 1 to get heartbeat debug messages.
    #SocketDebug 1       #Change this to 1 to get socket debug messagese.

Module Index | Import_generic Overview