#
Evanstrig Configuration File

(last revised 24 July, 1998)

    #
    #                  Evanstrig's Configuration File
    #
    MyModuleId    MOD_EVANSTRIG # module id for this program,
    InRing        WAVE_RING     # Transport ring to find waveform data on
    OutRing       PICK_RING     # Transport ring to write all output to
    LogFile       1

    HeartbeatInt  0     # Heartbeat interval (seconds)
                        # if 0, no heartbeats will be sent.

    Log_triggers 1      # If 1, log to screen only
                        # If 2, log to log file only
                        # If 3, log to screen and log file

    Debug_enabled  0    # If 1, print debug messages

    # List the message logos to grab from input transport ring
    #              Installation       Module       Message Type
    GetWavesFrom   INST_WILDCARD   MOD_WILDCARD   # TYPE_TRACEBUF msg

    # Define the maximum gap (in # of sample intervals) between
    # consecutive tracbuf messages to interpolate thru without a restart.
    # The number of samples that will be interpolated is MaxGap-1.
    MaxGap 3

    #  Magic numbers from John Evans for configuring the trigger:
    @evanstrig_params.d      # file with integer & floating-point parameters

    # Optional command for changing the maximum number of channels
    # which can be triggered on.  Default is 32.
    # MaxSCN 20

    # List the SCN's to trigger on:
    #           site  comp  net
    TriggerOn    MPR  VHZ  NC
    TriggerOn    MCM  VHZ  NC
    TriggerOn    MCV  VHZ  NC
    TriggerOn    MDC  VHZ  NC
    TriggerOn    MTU  VHZ  NC
    TriggerOn    SLK  VHZ  NN
    TriggerOn    MMP  VHZ  NC
    TriggerOn    MLM  VHZ  NC
    TriggerOn    MGP  VHZ  NC
    TriggerOn    MLK  VHZ  NC

Module Index | Evanstrig Overview