# ew2mseed Configuration File

(last revised May, 2003)

## 1. EXAMPLE CONFIGURATION FILE

    # Sample configuration file for ew2mseed
    # Version 0.8
    # I.Dricker  (i.dricker@isti.com)   15-May-2003

    #New field: StartLatency (15-May-2003)

    #New field: PriorityHighWater (02-Apr-2002)

    #New Field: LoopsBeforeService (02-Apr-2002)

    # New field: SocketReconnect (14-Mar-2001)

    # Note that the parameters are case sensitive

    # This defines the root directory where ew2mseed writes MiniSEED files

MseedDir ../mseed

    # Verbosity has five levels
    # 1 - minimal number of messages (default if verbosity omitted in configuration)
    # 2 - more verbose
    # 3 even more verbose
    # 4 high level of verbosity
    # 5 same as 4 plus addidng debug messages from ws_clienII.c WaveServer debug messages

    Verbosity 1

    # LogFile defines where to create log files
     #1 to log to disk;
     #0 to turn off disk logging;
     #2 to disable logging to stdout and stderr.

    LogFile 2

    # Optional : LockFile:
    # If not specified, no locking mechanism is provided
    # If a valid LockFile is defined, ew2mseed is prevented from
    # running multiple copies over a single ew2mseed.d

    LockFile ./ew2mseed.lock

    # SCNLocSz - List SCNs, location IDs, logical MSEED record size
    #       and compression algorithm to save in MiniSEED format.
    #
    # Note that record size must be a power of 2!!!
    #
    # NONE for the location code means that location code is non defined.
    # It will be replaced by two spaces in the binary MiniSEED header.
    # Compression algorithm: STEIM1 or STEIM2
    #

    #SCNLocSz BOSA BHZ GT cc  4096  STEIM1
    SCNLocSz  BMN BHZ LB NONE  512 STEIM2
    SCNLocSz  BLA BHZ US bb  2048 STEIM1
    SCNLocSz FLET EHZ LD NONE  1024 STEIM2
    #SCNLocSz CHIP EHZ LD aa  4096 STEIM2
    #SCNLocSz ARNY EHZ LD bb  4096 STEIM1
    #SCNLocSz PAL  EHE LD aa 4096 STEIM1

    #
    # OPTIONAL - specify StartTime. We are not interested in data before
    # this point. If this is not specified, ew2mseed will attempt to get all data
    # available in the tank.
    #
    # The format is mandatory and is yyyymnddhhmmss.00
    # where
    #        yyyy [4 chars] - year
    #        mn [2 chars] - month
    #        dd [2 chars] - day of month
    #        hh [2 chars] - hour of day
    #        mm [2 chars] - minutes
    #        ss [2 chars] - secs
    #        00 [2 chars] - usecs
    # THERE MUST be 17 symbols totally !
    #

    StartTime 20001119000000.00

    # Setup for WaveServers we'll interrogate:
    # list of IP addresses/names and ports of the  WaveServers we're to use

    # Multiple servers are OK!

    WaveServer 136.177.31.188 16022

    WaveServer the.other.one.gov 16023

    # We'll wait at most this long for the WaveServers
    # to respond to wsGertTraceBin() request.

    TravelTimeout  20

    # SocketReconnect defines how often (in seconds)
    # ew2mseed reconnects to the socket of WaveServerV.
    # the default value is 3600 s. It is safe to increase this number
    # if the link to the WaveServer is reliable.

# NOTE: parameter introduced 03/14/2001

    SocketReconnect  3000

    # OPTIONAL - RecordsNumber is a  number of MiniSEED records we are attempting to extract
    # in a single wsGetTraceBin() operation from the WaveServer.
    # Retrieval of more data from the server can result is faster throughput.
    # Keep in mind that there is a relation
    # between the number of records, the size of a records and the allocated
    # memory buffer, so  RecordsNumber * Record Size * 4 is approximately equivalent
    # to the size of memory buffer in bytes.
    # Make sure that you computer has enough memory to handle the request.
    # Larger values of RecordsNumber also require an increase of TravelTimeout parameter.
    # Default value for RecordsNumber is 1.

    RecordsNumber 5

#The next two fields are used for configuring a catch-up algorithm introduced in versions
#after April 2, 2002 (see http://mail.terra-bytes.org/ew2mseed/ew2mseed_cmd.html for detail)
#The first parameter is the maximum priority which can be assigned to the late channel (5 is default)
#The second parameters is the number of full loops over all channels before we enter the function
#which reassigns priorities depending on the channels' latencies. This number depends on the
#product of number of channels in ew2mseed configuration and the parameter "RecordNumber".
#We recommned to set the LoopsBeforeService parameter so that the Priority assignment function
#was hit every 30-60 minutes.

PriorityHighWater 6
LoopsBeforeService 20

#StartLatency parameter in hours is used to superseed StartTime parameter.
#The starttime is computed as the current time minus StartLatency and the
#resultanant number is used to compute StartTime. Either StartTime or StartLatency
#must be present in the configuration file. If both of them are present,
#the program will use the parameter which is below
#than the other one in the configuration file.
StartLatency 24

    #
    #       End of configuration

EarthWorm Module Index | ew2mseed overview

Contact: info@isti.com