#
scnl2scn Configuration File

(last revised 28 December 2006)

scnl2scn is a module to convert TRACEBUF2 into TRACEBUF messages by mapping SCNLs into SCNs.

BE VERY CAREFUL with this module as this could cause DUPLICATE WAVEFORM messages if 2 components have the same channel name but different location codes.

Below is a copy of the .d file with detailed notes on each parameter:

    #
    #                     Configuration file for scnl2scn
    #
    MyModuleId     MOD_SCNL2SCN  # Module id for this instance of scnl2scn,
    InRing         WAVE_RING     # Where to find input messages,
    OutRing        WAVE_RING2    # Where to put output messages,
                                 #  InRing and OutRing may be the same ring.
    HeartbeatInt   15            # Heartbeat interval in secs
                                 #   if 0, send no heartbeats
    Debug			     # Optional command, no parameters

    			     # logs every SCNL is sees!
    # List SCNL's that are to be converted and the SCN to which they are to be
    # renamed. Format is:
    # SCNL  sta chan net loc   sta chan net
    # You can list SCNL's explicitly or with wildcards. The only supported wildcard
    # for station and network names is "*"; no other characters should be included
    # in a station, network or location name if the wildcard is used.
    # For channel names, you can use "*" or two letters followed by `?', as in
    # "HH?". The `?' wildcard is supported only as the third character of the
    # channel name.
    #
    # The output SCN must be given explicitly if the input SCNL is given
    # explicitly.
    # If a wildcard is used in the input SCNL, you can use wildcards in the output.
    # In the output SCN, the wildcard means "use whatever was in the
    # input S, C or N".
    #
    # The explicit SCNL's will be sorted with scnl2scn starts up so that a binary
    # search can be used to quickly find a match.
    # Incoming packets will be matched against this explicit list first.
    # Any packets that don't match an explicit SCNL will then be matched against
    # the wildcarded SCNLs in the order they appear in this file.
    # Any packets that do not match the wildcard list WILL NOT BE CONVERTED.
    # To ensure that all packets are converted, you could end the SCNL list
    # with "SCNL * * * *  * * *". This will simply delete the location code from
    # any packets not otherwise matched.
    # Be careful with this, however. It may cause multiple SCNLs to be converted
    # into a single SCN, producing utter garbage!
    SCNL  * * * *  * * *

Module Index | scnl2scn Overview