Spectral Period Overloading Codes
EWDB_SM_PERIOD_PEAK_VALUE_CODE

Value: | -1
Description: | Identifies the motion as a peak type. Such as Peak Ground Acceleration(PGA), PGV, or PGD.

Strong Motion Message Query Types
EWDB_SM_SELECT_SMMESSAGES_W_CHANNEL_INFO

Value: | 2
Description: | Identifies a query that retrieves Strong Motion messages with channel and if available, event information.

EWDB_SM_SELECT_SMMESSAGES_W_CHANNEL_INFO_BY_EVENT

Value: | 3
Description: | Identifies a query that retrieves Strong Motion messages with channel and event info, only for messages that are associated with a given Event.

EWDB_SM_SELECT_SMMESSAGES_W_CHANNEL_INFO_WITHOUT_EVENT

Value: | 4
Description: | Identifies a query that retrieves Strong Motion messages with channel info, only for messages that are not associated with any Event.

EWDB_SM_SELECT_SMMESSAGES_W_ID_ONLY

Value: | 1
Description: | Identifies a query that retrieves only the IDs of Strong Motion messages(idSMMessage).

EWDB_SM_SELECT_SMMESSAGES_W_INFO

Value: | 0
Description: | Identifies a query that retrieves Strong Motion messages with message info only. (No channel or event information)

Strong Motion Motion Types
EWDB_SM_MOTION_TYPE_ACCELERATION

Value: | 1
Description: | Identifies a motion as acceleration.

EWDB_SM_MOTION_TYPE_DISPLACEMENT

Value: | 3
Description: | Identifies a motion as diplacement.

EWDB_SM_MOTION_TYPE_UNDEFINED

Value: | 0
Description: | Identifies an undefined type of motion. This type of motion is generally not supported.

EWDB_SM_MOTION_TYPE_VELOCITY

Value: | 2
Description: | Identifies a motion as velocity.