# Ringtocoax Configuration File Commands

(last revised 21 April 1999)
Page Index:
1. Example configuraton file
2. Functional command listing
3. Alphabetic command listing & description

On startup, ringtocoax reads the configuration file named on the command line. Commands in this file set up all parameters used in reading Earthworm messages from shared memory and broadcasting them onto ethernet as UDP packets. In the control file, lines may begin with a valid ringtocoax command (listed below) or with one of 2 special characters:

>     #  marks the line as a comment (example: # This is a comment).

>     @  allows control files to be nested; one control file can be
>        accessed from another with the command "@" followed by
>        a string representing the path name of the next control file
>        (example: @model.d).

Command names must be typed in the control file exactly as shown in this document (upper/lower case matters!).

## 1. EXAMPLE CONFIGURATION FILE

    #
    # This is ringtocoax's parameter file
    #
    # This program gets earthworm messages from a transport ring and broadcasts
    # them to ethernet.
    #
    #	*** WARNING ***
    #	This module does connection-less broadcasts.
    # 	In normal usage, it broadcasts onto an isolated, dedicated class b
    #	subnet. There must be no routing to or from that subnet.
    #	The broadcast is restricted to that subnet as stated below.
    #	Note that the companion module, coaxtoring, has strange
    #	system-specific addressing requirements

    MyModName         MOD_RINGTOCOAX  # Module id for this instance of ringtocoax
    RingName          WAVE_RING       # Shared memory ring for input/output
    LogSwitch         1               # 0 to completely turn off disk log file
    HeartBeatInterval 15              # Seconds between heartbeats
    MsgMaxBytes       4096            # Size of biggest message to be sent
    OutAddress        192.168.4.255   # IP address of net to broadcast to.
                                      # Set the node number to 255
                                      # eg. OutAddress    192.168.4.255
    OutPortNumber     2025            # Note: Under Solaris, if the port number
    				  # is at or below 1024,
                                      # ringtocoax must run as root.
    MaxLogo           256             # Maximum number of logos we can handle
                                      # Set to a number >= 0
    ScrnMsg           1               # If 1, print message logos on screen
                                      #    0, don't print logos.
    CopyStatus        1               # If 1, broadcast heartbeat and errors msgs.
                                      #    0, don't broadcast them.
    BurstInterval     10              # Sleep this many msec between bursts
    BurstCount        4               # Number of UDP packets per burst
    SqrtCount         2000            # Number of square roots between packets within a burst.

    # List each logo that you want to broadcast in a BroadcastLogo command.
    # If the BroadcastLogo command is omitted, all messages in RingName will
    # be shipped.
    #               installation   module_id     message_type
    #               ------------   ---------     ------------
    BroadcastLogo   INST_WILDCARD  MOD_WILDCARD  TYPE_TRACEBUF

## 2. FUNCTIONAL COMMAND LISTING

Below are the commands recognized by ringtocoax, grouped by the function they influence. All of the commands are required; they must be specified in the control file in order for ringtocoax to operate.

             Earthworm system setup:
    		HeartBeatInterval 	required
     		MyModName	   	required
    		RingName	   	required

    	Network Information:
    		OutAddress	   	required
    		OutPortNumber	   	required

    	Message Handling:
    		CopyStatus		required
    		MaxLogo			required
    		MsgMaxBytes	   	required
    		BurstInterval		required
    		BurstCount		required
    		SqrtCount		required
    		BroadcastLogo

    	Output Control:
    		ScrnMsg	   		required
    		LogSwitch		required

## 3. ALPHABETIC COMMAND LISTING & DESCRIPTION

In the following section, all configuration file commands are listed in alphabetical order. Listed along with the command (bold-type) are its arguments (in red), the name of the subroutine that processes the command, and the function within the module that the command influences. A detailed description of the command and is also given. Default values and example commands are listed after each command description.

    command arg1				processed by		function

    BroadcastLogo instid  modid  msgtype	ringtocoax_config	msg handling

> Specifies one message logo (instid, modid, and msgtype) to read from the shared memory region (named in the "RingName" command) and to broadcast onto ethernet. The instid must be a valid string in earthworm.h; modid and msgtype must be valid strings in earthworm.d. List one logo per "BroadcastLogo" command, and use as many commands as needed. If msgtype is TYPE_HEARTBEAT or TYPE_ERROR, be sure that the CopyStatus value is non-zero. If no "BroadcastLogo" command is given, ringtocoax defaults to broadcasting all messages in the designated shared memory region.

>     Example:  BroadcastLogo INST_MENLO MOD_WILDCARD TYPE_TRACEBUF

    BurstCount BurstCount			ringtocoax_config	msg handling

> Defines the number of UDP packets, BurstCount, in a broadcast "burst". Three commands, "BurstCount", "SqrtCount", and "BurstInterval", control the temporal spacing of UDP packets broadcast by ringtocoax. Ringtocoax broadcasts messages in groups of BurstCount packets; between the packets within a "burst", ringtocoax loops thru SqrtCount square root calculations to waste a little time. After broadcasting a "burst" of packets, ringtocoax sleeps for BurstInterval milliseconds, then it starts sending the next burst. The goal of spacing packets a tiny bit in time is to give the receiving program a better chance of catching every packet.

> UDP packets are variable in length up to a maximum of 1472 bytes (6 bytes of header, 1466 bytes of data). If an Earthworm message has a length less than or equal to 1466 bytes, it will be broadcast in a single UDP packet. If an Earthworm message is longer than 1466 bytes, it will be fragmented by ringtocoax, broadcast in multiple UDP packets, and reassembled by the receiving program (coaxtoring). Ringtocoax will never pack more than one Earthworm message in a single UDP packet.

> It is very important that the overall rate of broadcast is as at least as fast as the rate of local information production. For example, if your system produces 256 TYPE_TRACEBUF messages per second (464 bytes each = 1 UDP packet each), then the BurstCount, SqrtCount, and BurstInterval commands should be configured such that ringtocoax will broadcast at least 256 UDP packets per second. System clock resolution must be considered when configuring the three commands, especially BurstInterval. As of April 1999, the time resolution of each sleep on Windows NT is about 16 msec (one clock tick). On Solaris, the resolution is about 10 msec.

>     Default:  none
>     Example:  BurstCount 3

    BurstInterval BurstInterval			ringtocoax_config	msg handling

> Defines the minimum interval, in milliseconds, between "bursts" of UDP broadcasts. See the BurstCount command for a detailed description of ringtocoax's broadcasting scheme. BurstInterval must be a number greater than or equal to zero. Remember to consider the system clock resolution when configuring BurstInterval. As of April 1999, the clock-tick resolution is about 16 msec on Windows NT, and about 10 msec on Solaris.

>     Default:  none
>     Example:  BurstInterval 10

    CopyStatus CopyStatus				ringtocoax_config	msg handling

> Sets the CopyStatus switch to control whether ringtocoax broadcasts TYPE_ERROR and TYPE_HEARTBEAT messages. If no "BroadcastLogo" command is present, then ringtocoax will default to reading all messages in the shared memory region specified by the "RingName" command. If CopyStatus is non-zero, all of these messages will be broadcast onto ethernet. If CopyStatus is 0, TYPE_HEARTBEAT and TYPE_ERROR will not be broadcast, but all other messages will.

>     Default:  none
>     Example:  CopyStatus 0

    HeartBeatInterval nsec 			ringtocoax_config	Earthworm setup

> Defines the number of seconds nsec between TYPE_HEARTBEAT messages issued by ringtocoax.

>     Default:  none
>     Example:  HeartBeatInterval 15

    LogSwitch switch			ringtocoax_config	output

> Sets the on-off switch for writing a log file to disk. If switch is 0, no log file will be written. If switch is 1, ringtocoax will write a daily log file(s) called ringtocoaxxx.log_ccyymmdd where xx is ringtocoax's module id (set with "MyModName" command) and ccyymmdd is the current UTC date (ex: 19990123) on the system clock. The file(s) will be written in the EW_LOG directory (environment variable).

>     Default:  none

    MaxLogo nlogo				ringtocoax_config	msg handling

> Sets the maximum number, nlogo, of different message logos that ringtocoax can process. Ringtocoax assigns a sequence number (unsigned char) to each message based on its logo before it broadcasts the message. Space is allocated to store the last sequence number used for up to nlogo different logos. If the tracking arrays are full and ringtocoax gets a never-seen-before message logo from shared memory, ringtocoax will not broadcast that message, but it will issue a TYPE_ERROR message explaining the problem.

>     Default:  none
>     Example:  MaxLogo 256

    MsgMaxBytes nbytes			ringtocoax_config	msg handling

> Sets the size, in bytes, of the buffer that ringtocoax uses for storing Earthworm messages read from shared memory. nbytes should be the size of the largest message you expect ringtocoax to receive. If ringtocoax receives a message larger than nbytes, it will drop the entire message and issue a TYPE_ERROR message containing the string "too big for Buffer" and the logo of the dropped message.

>     Default:  none
>     Example:  MsgMaxBytes 51740

    MyModName mod_id			ringtocoax_config	Earthworm setup

> Sets the module id for labeling all outgoing heartbeat and error messages. mod_id is a character string (valid strings are listed in earthworm.d) that relates (in earthworm.d) to a unique single-byte number. All messages that ringtocoax receives from shared memory are tagged with their original logos when they are broadcast onto ethernet.

>     Default:  none
>     Example:  MyModName MOD_RINGTOCOAX

    OutAddress a.b.c.d			ringtocoax_config	network info

> Tells ringtocoax the TCP/IP address of the ethernet line onto which it should broadcast Earthworm messages. a.b.c.d is a character string in tcp/ip's standard dotted-decimal notation that ringtocoax uses along with the port number from the "OutPortNumber" command to set up a socket to which it will broadcast UDP Datagram packets. By convention, all Earthworm broadcasts have the node ("d" part of address) set to 255 (for example a.b.c.255).

>     Default:  none
>     Example:  OutAddress 192.168.4.255

    OutPortNumber port			ringtocoax_config	network info

> Defines the well-known port number port to be used by ringtocoax for broadcasting. port is an integer that ringtocoax uses along with the address from the "OutAddress" command to set up a socket to which it will broadcast UDP Datagram packets.
> NOTE: The port number must be greater than 1024. Smaller port numbers require root permission.

>     Default:  none
>     Example:  OutPortNumber 2025

    RingName ring				ringtocoax_config	Earthworm setup

> Tells ringtocoax which shared memory region to use for input/output. ring is a character string (valid strings are listed in earthworm.d) that relates (in earthworm.d) to a unique number for the key to the shared memory region. All messages that ringtocoax reads from shared memory are tagged with their original logos when they are broadcast onto ethernet.

>     Default:  none
>     Example:  RingName WAVE_RING

    ScrnMsg switch				ringtocoax_config	output

> Sets a switch for writing messages to the screen. If switch is 1, a line is printed to the screen detailing the logo and the sequence number of each Earthworm message broadcast to ethernet. If switch is 0, no messages are written to the screen.

>     Default:  none
>     Example:  ScrnMsg 0

    SqrtCount SqrtCount			ringtocoax_config	msg handling

> Defines the number of square root calculations ringtocoax performs between broadcasting each UDP packet of a "burst." See the BurstCount command for a detailed description of ringtocoax's broadcasting scheme. SqrtCount must be an integer greater than or equal to zero.

>     Default:  none
>     Example:  SqrtCount 2000

Module Index | Ringtocoax Overview