# Import_ida Configuration File

(last revised 17 March 1998)

    # @(#)import_ida.d	1.1 12/26/97
    # import_ida parameter file

    #  Basic Earthworm setup:

    MyModuleId         MOD_IMPORT_IDA # module id for this process
    OutRing            WAVE_RING      # output ring
    HeartBeatInterval  30             # seconds between heartbeats

    # We need to assign unique pin numbers to each net/sta/chan triple that
    # gets sent to the output ring.  Give the name of the file that contains
    # this information.  The format of this file must be the same as what
    # pick_ew expects.  You can create your own file with IDA specific
    # entries (see ida.sta for an example), or you can add the required
    # information to the pick_ew station file.  The picker parameters are
    # not required here, and as far as this program is concerned those fields
    # may be left blank.

    PinnoFile          ida.sta

    # It is up to the user to insure that there are entries in the above file
    # for all expected net/sta/chan triples, however the program will work even
    # if the database is incomplete.  In such a case, an unresolved net/sta/chan
    # will be assigned a default pin number of 12345.  You can override this
    # default by specifying an alternate value.

    DefaultPinno       12345

    # Define the policy to follow when reconnecting after circuit timeouts.
    # There are two choices: MINIMAL_GAP, or MINIMAL_DELAY.  If the former
    # is selected then the program will request the flow start at the end of
    # whatever has been received so far.  If the latter is selected then the
    # program will request the flow start with the most recent packet available
    # on the server.

    Policy             MINIMAL_DELAY

    # The network code for Project IDA stations is II, and that is the default
    # code which gets loaded into the packet headers.  If you want to override
    # this with some other code, enter it here.

    Network            II

    # List the server(s) and stream(s) that are desired.
    # The station channel specifications should follow the syntax
    # described in ftp://idahub.ucsd.edu:/pub/pickup/idatap-1.2.1.tar.Z
    #
    # You can give either the fully qualified host name, or its IP address
    # in the usual decmial dot notation (eg, 111.22.333.44)
    #
    #          Hostname              Station/channel list

    server   nnn.xxx.mmm.5        nna:bhz+pfo:bhz+sur:bhz

Module Index | Import_ida Overview