#
Fir Configuration File

(last revised 28 July, 2004)

    #
    #                     Configuration File for Fir
    #
    MyModId          MOD_FIR
    InRing           WAVE_RING       # Transport ring to find waveform data on,
    OutRing          WAVE_RING       # Transport ring to write output to,
                                     # InRing and OutRing may be the same.
    HeartBeatInterval     30         # Heartbeat interval, in seconds,
    LogFile            1             # 1 -> Keep log, 0 -> no log file
    #Debug		 		 # Write out debug messages (optional)

    MaxGap              1.5         # Maximum gap, in sample periods, allowed
                                    # between trace data points.
                                    # When exceeded, channel is restarted.

    # Specify the filter frequency response characteristics with two or more
    # commands fo the form: Band
    #
    # where:
    #   f_low = low frequency limit of a band
    #   f_high = high frequency limit of a band
    #   level = desired level of the band: 1 for pass band, 0 for stop band
    #   deviation = amount of ripple allowed from desired level
    #
    # All frequencies specified must be in the range 0.0 - 1.0, where 1.0
    # corresponds to the Nyquist frequency. (Nyquist frequency is half the sample
    # rate and is the maximum frequency content that can be in a time series.)
    # One band must start at 0.0 frequency; one band must end at 1.0 frequency. Any
    # number of additional bands may be specified (up to a total of ten bands.)
    Band 0.0 0.3 1 0.005
    Band 0.4 1.0 0 0.005

    # If you want Fir to compute and log its filter coefficients and then
    # exit, specify "TestMode".
    #TestMode

    #
    # Specify logos of the messages to grab from the InRing.
    # TYPE_TRACEBUF2 is assumed, therefore only module ID and
    # installation ID need to be specified
    #
    GetWavesFrom    INST_WILDCARD MOD_WILDCARD  # TYPE_TRACEBUF2 (assumed)

    #
    # List SCNL codes of trace messages to fir and their output SCNL codes
    # Wildcard characters are not allowed here.
    #
    #           IN-SCNL        OUT-SCNL
    GetSCNL TEST EHZ UW --  TEST EWZ UW 01

Module Index | Fir Overview