#
Import Generic Passive Configuration File

(last revised 5 July 2006)

## 1. EXAMPLE CONFIGURATION FILE

    #
    # import_gen_pasv configuration file
    #
    # The intent is that specific import_xxx modules can be cloned from this.
    # This program includes a site-specific routine "import_filter" which
    # determines what to do with the received messages. The default
    # "import_filter" routine assumes that the message originated from
    # an  "export_gen_pasv" with a default "export_filter" routine: That routine
    # attaches the logo of the originating message as the first nine characters
    # (3 groups of 3) of the outgoing message, and exports it.
    # The local "import_filter" removes this logo from the message, decodes it,
    # and broadcasts the message onto its ring under this logo.

     MyModuleId     MOD_IMPORT_GEN_PASV  # module id for this import,
     RingName       WAVE_RING            # transport ring to use for input/output,
     HeartBeatInt   30                   # internal heartbeat interval in seconds
    #
     LogFile        1                    # If 0, don't write logfile at all,

     MaxMsgSize     65000      	         # max size (bytes) for input/output msgs

    # Note: Messages are assumed to terminate with two newline '\n\n'
    #       characters. The '\n\n' are both removed, and replaced by a zero byte.
    #       Someday this should be an option defined in this file...
    # Note: If an oversized message is received, it will be discarded, the
    #       socket will be closed, log an error, and it will connect and try
    #	again. This might flood the log file if all incoming messages are
    #	too long. Maybe it should terminate instead...

     MyAliveString      "RCValive"       # heartbeat text to foreign server machine
     MyAliveInt         120              # seconds between alive msgs sent to server
                                         # 0 => no alive messages to sending machine

     ReceiverIpAdr      128.110.129.13   # Import data through this ethernet card
     ReceiverPort       16005            # IP port to set up for connections

    ### Sender description follows:

     SenderIpAdr        134.20.200.137   # The IP address of the export host

     SenderHeartRate    60	             # Sender's heart beat interval in seconds
    				                             # 0 => no heartbeat expected
     SenderHeartText    "SNDalive"       # Sender's heartbeat text
     SocketTimeout      60000            # Timeout for Socket_ew calls in mili secs
                                         # Should be atleast the SenderHeartRate
     HeartbeatDebug     0                # Optional: 1 = to get heartbeat debug msgs.
     SocketDebug        0                # Optional: 1 = to get socket debug msgs.

Module Index | Import_generic Overview