#
Heli_ewII Configuration File

(last revised May 1, 2006)

    #
    # This is the heli_ewII parameter file. This program gets data gulps
    # from the waveserver(s), and creates helicorder displays.
    # Derived from heli_ew and heli_standalone, which were derived from
    # Jim Luetgert's original efforts.

    # This program runs either standalone or as an Earthworm module.
    # If any of the four Earthworm paramaters below are stated, it will asssume
    # that it's supposed to be a module. It will beat it's heart into the ring,
    # and use the Earthworm logging scheme. Other wise, it runs standalone.
    LogSwitch 1
    MyModuleId MOD_HELI_EWII
    RingName ASSOC_RING
    HeartBeatInt	10

    wsTimeout 30 # time limit (secs) for any one interaction with a wave server.

    # List of wave servers (ip port comment) to contact to retrieve trace data.
     WaveServer 136.177.31.188 16022      "harry"

    # Directory in which to store the temporary .gif, .link and .html files.
    GifDir   C:\alex\heli_alex\Gifs\

    # Plot Parameters - sorry it's so complex, but that's the price of versatility
            # The following is designed such that each SCN creates it's own
            # helicorder display; one per day of data.
    # S                  Site
    # C                  Component
    # N                  Network
    # L 	             Location
    # 04 HoursPerPlot    Total number of hours per gif image
    # 05 Plot Previous   On startup, retrieve and plot n previous hours from tank.
    # 06 Local Time Diff UTC - Local.  e.g. -7 -> PDT; -8 -> PST
    # 07 Local Time Zone Three character time zone name.
    # 08 Show UTC        UTC will be shown on one of the time axes.
    # 09 Use Local       The day page will be local day rather than UTC day.
    # 10 XSize           Overall size of plot in inches
    # 11 YSize           Setting these > 100 will imply pixels
    # 12 Minutes/Line    Number of minutes per line of trace
    # 13 Gain Factor     Instrument gain in microvolt/bit.
    # 14 Scale Factor    Scale factor to dress up image.
    # 15 Mean Removal    Mean of 1st minute of each line will be removed.
    # Comment            A comment for the top of the display.
    #
    #     S    C   N  L 04 05  06  07   08 09 10  11  12 13   14   15  Comment

     Plot AHID BHE US -- 12 1   -8  PST  1  0  20  20  15 0.1  1.5  1   "Alston BPA"
     Plot ADK  SHZ AT -- 12 1   -8  PST  1  0  20  20  15 0.1  1.5  1   "Mt. Rainier Summit"

        # *** Optional Commands ***

     Days2Save     7    # Number of days to display on web page; default=7
    # Actually, "Days2Save" is really the number of GIFs of each SCN to save.
    # For example, if HoursPerPlot is 12, you will save 7 gifs for 3.5 days.

     UpdateInt    10    # Number of minutes between updates; default=2
     RetryCount    2    # Number of attempts to get a trace from server; default=2
    # Logo    smusgs.gif # Name of logo in GifDir to be plotted on each image

    # We accept a command "Clip" which sets trace clipping at this many
    # vertical divisions
    Clip 5

    # We accept a command "SaveDrifts" which logs drifts to GIF directory.
    # SaveDrifts

    # We accept a command "Make_HTML" to construct and ship index HTML file.
    Make_HTML

    # We accept a command "IndexFile" to name the HTML file.
    # Default is "index.html"
    IndexFile welcome.html

    # We accept a command "BuildOnRestart" to totally rebuild images on restart.
    BuildOnRestart

    # We accept a command "Debug" which turns on a bunch of log messages
    Debug
    WSDebug

Module Index | Heli_ew Overview