#
Decimate Configuration File

(last revised 17 October, 1999)

    #
    #                     Configuration File for decimate
    #
     MyModId         MOD_DECIMATE
     InRing             WAVE_RING    # Transport ring to find waveform data on,
     OutRing            WAVE_RING    # Transport ring to write output to,
                                     # InRing and OutRing may be the same.
     HeartBeatInterval  30           # Heartbeat interval, in seconds,
     LogFile            1            # 1 -> Keep log file, 0 -> no log file
                                     # 2 -> log to file but not to stderr/stdout
    #Debug		 		 # Write out debug messages (optional)

    # Specify the decimation rates as one or more integer values greater than 1,
    # all on one "DecimationRates" line, enclosed in quotes.
    # These will be used in successive stages of decimation. The overall
    # decimation rate is the product of all the stage decomation rates.
    # The filters will be more efficient if several small decimation stages
    # are used instead of one large one, and if largest rates are given first.
    # Currently a maximum of 10 stages is enforced.
    #--------------------------------------------------------------------------
     DecimationRates    "5 2"     # Decimation rates of each stage, in quotes!

     MinTraceBuf         10       # Minimum number of samples in output TRACE_BUF.

     MaxGap              1.5      # Maximum gap, in sample periods, allowed
                                  # between trace data points.
                                  # When exceeded, channel is restarted.

    #TestMode                     # If you want Decimate to compute and log
                                  # its filter coefficients and then
                                  # exit, specify "TestMode".

    # Specify logo(s) of the messages to grab from the InRing.
    # Up to 10 GetWavesFrom commands may be used.
    # Must specify installation ID, module ID and message type.
    # Installation and module may be wildcarded.
    # The only valid messages types are TYPE_TRACEBUF and TYPE_TRACEBUF2
    # Output message type will be the same as the input message type.
    #--------------------------------------------------------------------------
     GetWavesFrom    INST_WILDCARD MOD_WILDCARD TYPE_TRACEBUF2

    # List SCNL codes of trace messages to decimate and their output SCNL codes.
    # If old GetSCN command is used, input/output location codes are set to "--".
    # Wildcard characters are not allowed here.
    #--------------------------------------------------------------------------
    #         Input-SCNL      Output-SCNL
     GetSCNL  ABC EHZ UW --   ABC EWZ UW 01

Module Index | Decimate Overview