#
scnl2scn Configuration File

(last revised 1 June 2006)

scnl2scn is a module to convert TRACEBUF2 into TRACEBUF messages by stripping off the location code.

BE VERY CAREFUL with this module as this could cause DUPLICATE WAVEFORM messages if 2 components have the same channel name but different location codes.

Below is a copy of the .d file with detailed notes on each parameter:

    #
    #                     Configuration file for scnl2scn
    #
    MyModuleId     MOD_SCNL2SCN  # Module id for this instance of scnl2scn,
    InRing         WAVE_RING     # Where to find input messages,
    OutRing        WAVE_RING2    # Where to put output messages,
                                 #  InRing and OutRing may be the same ring.
    HeartbeatInt   15            # Heartbeat interval in secs
                                 #   if 0, send no heartbeats

Module Index | scnl2scn Overview