#
Heli_ew Configuration File

(last revised August 10, 1999)

    #

    # This is the heli_ew parameter file. This module gets data gulps

    # from the waveserver(s), and creates helicorder displays.

    #  Basic Earthworm setup:

    #

    LogSwitch    1              # 0 to completely turn off disk log file

    MyModuleId   MOD_HELI       # module id for this instance of report

    RingName     HYPO_RING      # ring to get input from

    HeartBeatInt 15             # seconds between heartbeats

    # List the message logos to grab from transport ring

    #             Installation     Module        Message Type

    GetSumFrom    INST_WILDCARD    MOD_EQPROC    TYPE_HINVARC

    wsTimeout 12 # time limit (secs) for any one interaction with a wave server.

    # List of wave servers (ip port comment) to contact to retrieve trace data.

     WaveServer aaa.bbb.ddd.eee 16022      "wsv2 - ad1"

     WaveServer aaa.bbb.ddd.fff 16023      "wsv2 - ad2"

    # List of target computers/directories to place output.

    #       UserName  IP Address            Directory

    Target myname@webserver1:/home/www/waveforms/helicorder/

    Target myname@webserver2:/home/www/waveforms/helicorder/

    # Filename prefix on target computer.  This is useful for identifying

    # files for automated deletion via crontab.

    Prefix nc

    # Directory in which to store the temporary .gif, .link and .html files.

    GifDir   /home/bigfiles/GIFs/helicorder/

    # Plot Parameters - sorry it's so complex, but that's the price of versatility

            # The following is designed such that each SCN creates it's own

            # helicorder display; one per day of data.

    # S                  Site

    # C                  Component

    # N                  Network

    # 04 XSize           Overall size of plot in inches

    # 05 YSize           Setting these > 100 will imply pixels

    # 06 Minutes/Line    Number of minutes per line of trace

    # 07 Gain Factor     Instrument gain in microvolt/bit.

    # 08 Scale Factor    Scale factor to dress up image.

    # 09 Plot Previous   On startup, retrieve and plot n previous hours from tank.

    # 10 Local Time Diff UTC - Local.  e.g. -7 -> PDT; -8 -> PST

    # 11 Local Time Zone Three character time zone name.

    # 12 Show UTC        UTC will be shown on one of the time axes.

    # 13 Use Local       The day page will be local day rather than UTC day.

    # 14 Mean Removal    Mean of 1st minute of each line will be removed.

    # Comment            A comment for the top of the display.

    #

    #     S    C   N  04  05  06 07   08   09  10  11   12 13 14  Comment

     Plot MSL  VHZ NC 10  20  15 1.0  1.0  1   -7  PDT  1  0  1   Mammoth

     Plot HSF  VHZ NC 10  20  15 0.5  1.0  1   -7  PDT  1  0  1   "San Juan Bautista"

     Plot GPM  VHZ NC 10  20  15 0.5  1.0  1   -7  PDT  1  0  1   "Geysers"

     Plot KRP  VHZ NC 10  20  15 0.25 1.0  1   -7  PDT  1  0  1   "Cape Mendocino"

     Plot JSF  VDZ NC 10  20  15 6.8  1.0  1   -7  PDT  1  0  1   "Bay Area DST"

     Plot JSG  VDZ NC 10  20  15 1.0  1.0  1   -7  PDT  1  0  1   "Bay Area Nano"

        # *** Optional Commands ***

     Days2Save     7    # Number of days to display on web page; default=7

     UpdateInt    10    # Number of minutes between updates; default=2

     RetryCount    2    # Number of attempts to get a trace from server; default=2

     Logo    smusgs.gif # Name of logo in GifDir to be plotted on each image

    # We accept a command "SaveDrifts" which logs drifts to GIF directory.

      SaveDrifts

    # We accept a command "Debug" which turns on a bunch of log messages

    # Debug

    # WSDebug

Module Index | Heli_ew Overview