# WinSDR to Earthworm for EW Version 7.0 Configuration File

Created July 10, 2006 by Larry Cochrane

Below is a typical ws2ew.d configuration file. This file should be located in the \earthworm\run\params directory. The ModuleId must be added to the earthworm.d file also located in this directory.

    #
    #                    CONFIGURATION FILE FOR WS2EW
    #                    -----------------------------
    ModuleId         MOD_WS2EW_A    # Module id of this instance of Ws2Ew
    OutRing          WAVE_RING      # Transport ring to write waveforms to
    Host             10.0.0.10      # Host name or IP address of the system running WinSDR
    Port             16064          # Port number to use when connecting to WinSDR
    HeartbeatInt     15             # Heartbeat interval in seconds
    AdcDataSize      2              # ADC trace buffer data size in bytes. Can be 2 or 4 bytes
    #
    #                        OPTION PARAMETERS
    SocketTimeout   60              # Socket timeout in seconds (default = 60)
    RestartWaitTime 60              # Seconds to wait between reconnects (default = 60)
    NoDataWaitTime  45              # Seconds to wait before resetting connection
    NoHostMessages  1               # If 1 log messages from the host will not be processed (default = 0)
    #
    #                        CHANNEL CONFIGURATION
    Nchan            8              # Number of channels running on the host WinSDR system
    ChanRate         100            # Sampling rate of the WinSDR system
    #
    #
    #     SCNL (Station/Component/Network/Location) VALUES FOR EACH DAQ CHANNEL
    # Chan lines must follow the Channel Configuration lines in this file.
    #
    #     DAQ      Station/
    #   Channel    Comp/Net/Loc    Send to Earthworm
    #   -------   --------------   -----------
    Chan    0     PSN1 BHZ PN NC       YES
    Chan    1     PSN1 BHN PN NC       NO
    Chan    2     PSN1 BHE PN NC       YES
    Chan    3     PSN1 LHZ PN NC       YES
    Chan    4     PSN1 LHN PN NC       NO
    Chan    5     PSN1 LHE PN NC       NO
    Chan    6     PSN1 SHZ PN NC       NO
    Chan    7     PSN1 SHN PN NC       YES
    #

WinSDR to Earthworm Overview