[Date Prev][Date Next][Thread Prev][Thread Next][Date Index][Thread Index]

# Earthworm V5.1 is released.

- To: earthw-list@nmt.edu
- Subject: Earthworm V5.1 is released.
- From: Barbara Bogaert <bogaert@usgs.gov>
- Date: Wed, 04 Oct 2000 17:47:05 -0600

    Earthworm V5.1 Release
    10/4/00

    V5.1 Is Released
    ****************
    It can be retrieved from the Earthworm ftp site
    ghtftp.cr.usgs.gov/pub/OUTGOING/earthworm/release_v5.1

    New Features of EW V5.1
    ***********************
    k2ew: Communicates with the K2 data logger from Kinemetrics. Uses TCP or
    COM port for communication on WindowsNT, TCP or TTY (serial) comms on Unix.
    See src/data/sources/k2ew/Doc or the Earthworm web pages for documentation.

    ringdup: Program to read messages (with user given logos) from one ring and
    deposit them in another. This is mainly copied
    from export. This is actually two programs: ringdup_generic and ringdup_scn.

    naqs2ew: Interfaces with the Nanometrics digital data acquisition program,
    NaqsServer, requests continuous waveform data
    from a list of SCNs and outputs Earthworm tracebuf packets into an
    Earthworm transport ring.

    Event Review Using the Earthworm Database: The Event Review provides
    Earthworm with a remote, rapid event review
    capability. Its intended use is permit a duty seismologist to rapidly
    respond to a significant event. It was NOT designed to
    serve as a routine analysis facility.

    CONTRIBUTED SOFTWARE
    **************************

    The contributed software can be found at
             ghtftp.cr.usgs.gov/pub/OUTGOING/earthworm/contributed_software
    Coming Soon: A table describing contributed software can be found at URL:
    www.cnss.org/EWAB/Contributed/Contributed.htm

    UNIVERSITY OF UTAH SEISMIC STATION:
    IMPORT_GEN_PASV/EXPORT_ACTV: The original Earthworm import/export pair have
    been modified such that import_generic is now passive and the export
    modules now initiates communication. import_gen_pasv module prepares a port
    and waits for a connection request from a export_actv module. These modules
    will become part of the core Earthworm in release v5.2.

    Barbara Bogaert                 U.S. Geological Survey
    Project Manager, Earthworm Development Group
    bogaert@usgs.gov                        phone:  303-273-8491

- Prev by Date: anss-ma update
- Prev by thread: anss-ma update
- Index(es):
  - Date
  - Thread