#
Evansassoc Configuration File

(last revised August 10, 1999)

    #
    #           evansassoc's Configuration File
    #
    MyModuleId       MOD_EVANSASSOC    # Module id for this program,
    InRing           PICK_RING         # Transport ring to find triggers on
    OutRing          HYPO_RING         # Transport ring to write output to
    HeartbeatInt     30                # Heartbeat interval (s); 0=no heartbeat
    LogFile          1                 # 1=write log file on disk; 0=don't

    # List the message logos to grab from transport ring
    #                Installation       Module       Message Type
    GetTriggersFrom  INST_WILDCARD   MOD_WILDCARD      # trigger

    # LP-trigger association parameters:
    TriggerTimeLimit  17    # seconds; Set to (array aperture)/(8 or 10 km/s).
    CriticalMu        10    # number of triggers within TriggerTimeLimit.
    CriticalNu        10    # ..."... Set equal to CriticalMu.

    # Parameters for saving seismograms:
    MinEventTime     90     # total record length (s) of "normal" event
    MaxEventTime    105     # total record length (s) of "big" event
    PreEventTime     15     # pre-event portion (s) of event record

    EventIDfile  nextlp.id  # name of file containing next valid eventid
                            # this file should live in EW_PARAMS directory

    # List any other channels (time code, non-seismic, etc) that should be
    # included in every event message. Wildcards (*) may be used in any field.
    # List one SCN per line, as many as you need:
    #           sta chan network
    AddChannel  MSL  VHZ  NC
    AddChannel  MDR   *   NC

Module Index | Evansassoc Overview