Main Page Class Hierarchy Compound List File List Compound Members File Members

# ew2rsam.h

Go to the documentation of this file.

    00001
    00002 /*
    00003  *   THIS FILE IS UNDER RCS - DO NOT MODIFY UNLESS YOU HAVE
    00004  *   CHECKED IT OUT USING THE COMMAND CHECKOUT.
    00005  *
    00006  *    $Id: ew2rsam_8h-source.html,v 1.1 2006/05/19 16:55:01 paulf Exp $
    00007  *
    00008  *    Revision history:
    00009  *     $Log: ew2rsam_8h-source.html,v $
    00009  *     Revision 1.1  2006/05/19 16:55:01  paulf
    00009  *     first inclusion
    00009  *
    00010  *     Revision 1.1  2000/02/14 20:05:54  lucky
    00011  *     Initial revision
    00012  *
    00013  *
    00014  */
    00015
    00016 /*
    00017  * ew2rsam.h
    00018  *
    00019  *   Header file for the ew2rsam module
    00020  *   Defines local data structure used for book-keeping
    00021  *
    00022  *   Lucky Vidmar Thu May  6 10:07:21 MDT 1999
    00023  *
    00024  */
    00025
    00026
    00027 #define DC_ARRAY_ENTRIES        24
    00028 #define DC_TIME_DIFF            2.56
    00029 #define DC_STARTUP_ENTRIES      5
    00030 #define DC_OFFSET_INVALID       -1.00
    00031 #define TIME_INVALID        -1.00
    00032 #define MAX_TIME_PERIODS        5
    00033
    00034 typedef struct time_period_struct
    00035 {
    00036         double  time_period;    /* time period in seconds */
    00037         double  rsam_value;             /* currently kept rsam total */
    00038         int             rsam_nsamp;             /* samples in the current total */
    00039         double  rsam_starttime; /* when did we start counting ? */
    00040
    00041 } Tstruct;
    00042
    00043 /* there will be one for each requested channel */
    00044 /* with the maximum read from the configuration file */
    00045
    00046 typedef struct rsam_values_struct
    00047 {
    00048
    00049         /* START DC offset section */
    00050
    00051         double  DC_offset;                      /* DC offset value */
    00052
    00053         double  DC_cur_val;                     /* Current DC total */
    00054         int             DC_cur_nsamp;           /* Number of samples in current total */
    00055         double  DC_starttime;           /* When did we start counting ? */
    00056
    00057         double  DC_array[DC_ARRAY_ENTRIES];     /* Averages for previous time slices */
    00058         int             DC_cur_pos;                     /* index of the current position in the array */
    00059         int             DC_start_pos;           /* index of the starting position in the array */
    00060
    00061         int             DC_startup;                     /* TRUE if we are still starting out */
    00062         /* END DC offset section */
    00063
    00064         /* START time period section */
    00065         Tstruct         TP[MAX_TIME_PERIODS];
    00066
    00067 } RSAM_val;
    00068
    00069
    00070 typedef struct rsam_struct
    00071 {
    00072
    00073         char    sta[7];
    00074         char    chan[9];
    00075         char    net[9];
    00076         RSAM_val *values;
    00077
    00078 } RSAM;
    00079