## Virginia Tech Regional Seimic Network, CA

Date: March 6, 1998

### Location, Contact, and Address:

Virginia Tech Seimological Observatory
Department of Geological Sciences
Virginia Polytechnic Institute and State University
Blacksburg, Va 24061

#### Earthworm Contact:

- Martin Chapman (chapman@vtso.geol.vt.edu) 540-231-5036
- Arthur Snoke (Snoke@equake.geol.vt.edu) 540-231-6028

### Network Characteristics:

- 9 short Period stations (21 channels).
- 2 Broadband recording systems at Blacksburg, Va.
- 24-bit continuous digital telemetry from 5 stations.
- continuous analog telemetry from 3 stations, digitized and recorded in event triggered mode.

###

### Standard Earthworm Modules Currently in Use

Basic earthworm system was installed in winter of 1997, for connection to NSN through VDL; however the system has never worked properly.

### Earthworm Needs:

Technical support and guidance from the Earthworm Community

### Goals:

Our goal is to interface our on-site Earthworm with our RefTek acquisition system and analog data steams.

Return to main Earthworm or Sites pages.