# Earthworm Modules:
geqproc Configuration File Commands

(last revised June 6, 2006)

    # Configuration file for geqproc
    #
    # Alternate head of mega-module not unlike eqproc or eqprelim.
    # We pick up TYPE_LOC_GLOBAL from the input ring (as output by global_proc),
    # convert to TYPE_HYP2000ARC, and then pass along the pipe.  There
    # is no throttle or waiting to make sure this is the "final" version
    # as that task is assumed to be performed elsewhere such as in global_proc.
    #
    # Note also that we throw out any arrivals not suitable for Hypo (e.g. depth
    # phases).  This is dangerous and could result in a solution considerably
    # less accurate than the original.  It is concommitant upon the user to
    # assure that geqproc is attached to a ring that only has global loc
    # messages for areas with dense station coverage for which picks are
    # included in the incoming message.  eqfilterII may be used for this task.

    LogFile 1     # 0 means don't create a disc log file. 1=> do.
                  # 2 means write to module log but not to stderr/stdout
    MyModuleId MOD_GEQPROC
    InRing     GLOBAL_RING
    OutRing    HYPO_RING
    HeartBeatInt 30
    PipeTo "eqbuf eqbuf.d"

    #
    # Optional Debug switch - if this is uncommented
    # lots of debug messages will be produced
    #
    Debug

    # What message logos to listen to. Can be more than one, but no more
    # than five.
    # The type is one of TYPE_LOC_GLOBAL, no choice

    GetEventsFrom INST_WILDCARD MOD_GLOBALPROC # TYPE_LOC_GLOBAL

Module Index | Glass Overview