#
Compress_UA Configuration File

(last revised 9 July, 2002)

    #     compress_UA's Configuration File
    #
    MyModId       MOD_COMPRESS_UA   # This instance of compress_UA
    InRing              WAVE_RING   # Transport ring to find waveform data on,
    OutRing             COMP_RING   # Transport ring to write output to,
    HeartBeatInterval   15          # Heartbeat interval, in seconds,
    LogFile             1           # 0=write log to stderr/stdout, not to disk
                                    # 1=write a log file to disk
                                    # 2=write a module log but not to stderr/stdout

    UseOriginalLogo     0   # 0=use compress_UA's logo on outgoing TYPE_TRACE_COMP_UA msgs
                            # non-zero=use instid & modid of original TYPE_TRACEBUF msg
                            #          on outgoing TYPE_TRACE_COMP_UA msg

    # instead of getting specific LOGOS, we are only interested in
    # messages of TYPE_TRACEBUF, but we may want to specify messages
    # with particular SCN codes of interest
    #
    # Wildcard character '*' is allowed in the SCN_Code fields
    #

    #GetEventsFrom  *   *   *       INST_WILDCARD      MOD_WILDCARD
     GetEventsFrom  *   *   NC      INST_WILDCARD      MOD_WILDCARD
     GetEventsFrom  KSP *   *       INST_WILDCARD      MOD_WILDCARD
    #GetEventsFrom  KSP *   NC      INST_WILDCARD      MOD_WILDCARD
    #GetEventsFrom  KSP VHZ *       INST_WILDCARD      MOD_WILDCARD
    #GetEventsFrom  HGS VHZ NC      INST_WILDCARD      MOD_WILDCARD

Module Index | Compress/Decompress Overview