#
Decompress_UA Configuration File

(last revised 10 July, 2002)

    #
    #          Configuration File for decompress
    #
    MyModId     MOD_DECOMPRESS_UA   # This instance of pick_ew
    InRing              COMP_RING   # Transport ring to find compressed data on,
    OutRing             WAVE_RING   # Transport ring to write output to,
    HeartBeatInterval   15          # Heartbeat interval, in seconds,
    LogFile             1           # 0=write log to stderr/stdout, not to disk
                                    # 1=write a log file to disk
                                    # 2=write a module log but not to stderr/stdout

    GetWavesFrom  INST_WILDCARD MOD_WILDCARD  # only looks for msgtype:TYPE_TRACE_COMP_UA

    UseOriginalLogo     0           # 0=use decompress_UA's logo on outgoing TYPE_TRACEBUF msgs
                                    # non-zero=use instid&modid of original compressed msg
                                    #          on outgoing TYPE_TRACEBUF msg

Module Index | Compress/decompress Overview