# Eqverify_Assemble Configuration File Commands

(last revised 22 June 2009)

    #
    # This is eqverify_assemble's parameter file
    #
    MyModuleId  MOD_EQPROC  # module id to label logfile  with.
                            # Note: eqverify_assemble is part of a mega-module
                            # which is ultimately started by the program eqproc.
                            # All child processes of this mega-module need to use
                            # the same module id (thus use eqproc's module id).
    LogFile       1         # 0=no log; 1=log errors
                            # 2=write to moduel log but not to stderr/stdout
    # send output to the following command:
     PipeTo "log_everything"
    # PipeTo "hypo_mgr hypo_mgr.d ncal.hyp"

    # Required commands to turn glitch tests on or off.
    # Specify the minimum version (from eqassemble) for
    # which a test should be run.
    # eqassemble versions are: Prelim: 0; Rapid: 1; Final: 2
    # specify 3 to turn off a test for all versions
    test_slopevsmag  2
    test_freefitrms  2
    test_codawt      2
    test_pgroup      1

    # event weight at which event is "noise" for Prelim (version 0),
    # Rapid (version 1) or Final (version 2) reports from eqassemble
    PrelimThreshold     1
    RapidThreshold	    1
    FinalThreshold	    3

    # Optional commands that change eqverify_assemble test defaults
    # force_report  18 2.0    # report events with more than 18 picks
    #                         # and mag>=2.0 regardless of event weight
    # define_glitch  4 0.03   # a glitch is at least 4 picks within
                              # 0.03 seconds
    # MaxDeltaT         30.   # consider arrival times within this many
    #                         # seconds of the 1st arriving pick
    # coda_clip        820    # level at which a coda-avg-absolute-value
    #                         # is clipped (see notes in eqcoda.command)

Module Index | Glass Overview