#
pick_recorder Configuration File

(last revised Sept 1, 2006)

pick_recorder is a utility for reading in messages from a file (in binary form) and injecting them into a ring.

Below is a copy of the .d file with detailed notes on each parameter

    #
    #                     Configuration File for pick_recorder
    #
    MyModId        MOD_PICK_RECORDER
    InRing           PICK_RING       # Transport ring to find PICK data on,
    HeartBeatInterval     15         # Heartbeat interval, in seconds,
    LogFile                1         # 1 -> Keep log, 0 -> no log file
                                     # 2 to log to module log but not to stderr/stdout
    #Debug           0               # OPTIONAL,  0-no debug
                                     #            1-basic debug
                                     #            2-super debug

    #
    # Specify logos of the messages to grab from the InRing.
    # TYPE_PICK2K and TYPE_PICK_SCNL are assumed, therefore only module ID and
    # installation ID need to be specified. Specify as many as necessary.
    #
    GetPicksFrom    INST_WILDCARD MOD_WILDCARD  # TYPE_PICK2K (assumed)

    #
    # TargetDir - directory where picks will be written
    #
    TargetDir ./pick_dir

Module Index | pick_recorder Overview